
**RFC-LFP002\_v2**


**Suggested problem**  
The inputs SALW, OILAPI, GOR, SGG\_O, and SGG\_G have currently Location = Interval in 2018\_lfp\_fluidparameters.lls as shown in Figure 1.

  
Figure 1. Interval inputs for SALW, OILAPI, GOR, SGG\_O, and SGG\_G.

**Suggested solution**

Change the Location from Interval to Log for SALW, OILAPI, GOR, SGG\_O, and SGG\_G.

**Spelling mistake**



**Reference**

N/A